;This .inf file is a modified version of the example INF provided
;in the Microsoft document:
;"How to Use WinUSB to Communicate with a USB Device"


[Version]
Signature = "$Windows NT$"
Class = CustomUSBDevices
ClassGuid= {a503e2d3-a031-49dc-b684-c99085dbfe92}
Provider = %MFGNAME%
DriverVer=10/12/2010,1.0.0.3
CatalogFile=MCHPWinUSBDevice_v2.cat	;CAT file used when obtaining a WHQL signature on the driver package
					;Otherwise isn't needed.
;------------------------------------------------------------------------------
; ========== Manufacturer/Models sections ===========
;------------------------------------------------------------------------------
[Manufacturer]
%MFGNAME% = MyDevice_WinUSB,NTx86,NTamd64

;------------------------------------------------------------------------------
;  Vendor and Product ID Definitions
;------------------------------------------------------------------------------
; When developing your custom USB device, the VID and PID used in the PC side
; application program and the firmware on the microcontroller must match.
; Modify the below lines to use your VID and PID.  Use the format as shown below.
; Note: One INF file can be used for multiple devices with different VID and PIDs.
; For each supported device, append ",USB\VID_xxxx&PID_yyyy" to the end of the line.
; There is a maximum number of devices that can be supported per line however.
; If you append a large number of VID/PIDs to the end of the line, and get a:
; "The data area passed to a system call is too small." error when trying to install
; the INF, try removing some of the VIDs/PIDs.
;------------------------------------------------------------------------------
[MyDevice_WinUSB.NTx86]
%DESCRIPTION% =USB_Install, USB\VID_04d8&PID_ef08

[MyDevice_WinUSB.NTamd64]
%DESCRIPTION% =USB_Install, USB\VID_04d8&PID_ef08


;=========================================================================================
;ClassInstall32 and ClassInstall_AddReg sections used to make new device manager category.
;=========================================================================================
[ClassInstall32]
AddReg=ClassInstall_AddReg

[ClassInstall_AddReg]
HKR,,,,%DEVICEMANAGERCATEGORY%
HKR,,Icon,,"-20"


; =================== Installation ===================

[USB_Install]
Include=winusb.inf
Needs=WINUSB.NT

[USB_Install.Services]
Include=winusb.inf
AddService=WinUSB,0x00000002,WinUSB_ServiceInstall

[WinUSB_ServiceInstall]
DisplayName     = %WinUSB_SvcDesc%
ServiceType     = 1
StartType       = 3
ErrorControl    = 1
ServiceBinary   = %12%\WinUSB.sys

[USB_Install.Wdf]
KmdfService=WINUSB, WinUsb_Install

[WinUSB_Install]
KmdfLibraryVersion=1.9

[USB_Install.HW]
AddReg=Dev_AddReg

[Dev_AddReg]
HKR,,DeviceInterfaceGUIDs,0x10000,"{58D07210-27C1-11DD-BD0B-0800200C9a66}"
;When editing the GUID (the big hex number with dashes inside the squiggly 
;braces), make sure to write the intended PC application to use the same GUID.
;Otherwise the application won't be able to find the USB device properly.

[USB_Install.CoInstallers]
AddReg=CoInstallers_AddReg
CopyFiles=CoInstallers_CopyFiles

[CoInstallers_AddReg]
HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"

[CoInstallers_CopyFiles]
WinUSBCoInstaller2.dll
WdfCoInstaller01009.dll

[DestinationDirs]
CoInstallers_CopyFiles=11

; ================= Source Media Section =====================

[SourceDisksNames]
1 = %DISK_NAME%,,,\i386
2 = %DISK_NAME%,,,\amd64

[SourceDisksFiles.x86]
WinUSBCoInstaller2.dll=1
WdfCoInstaller01009.dll=1

[SourceDisksFiles.amd64]
WinUSBCoInstaller2.dll=2
WdfCoInstaller01009.dll=2

; =================== Strings ===================

[Strings]
MFGNAME="Microchip Technology, Inc."
DESCRIPTION="Microchip WinUSB Device"
WinUSB_SvcDesc="WinUSB Device"
DISK_NAME="WinUSB Device Install Disk"
DEVICEMANAGERCATEGORY="Custom USB Devices"

